#### Triskel Christchurch

#### Technical Information (as of November 2023)

#### STAGE:

* 6m x 5m x .6m (Clearance 6m)
* 2 x 8ft x 4ft Risers with 1ft and 2ft Legs

#### SOUND DESK:

* Midas M32 with 1xDL32 Stagebox

#### PA:

* 4 x Nexo GEO S1230 (on Downstage truss)
* 2 x Nexo GEO RS18 (2×18”) Subs
* 1 x Nexo NXAMP 4×4 Control Amp

#### MONITORS:

* 6 x Nexo PS10s
* 1 x Nexo 15″ Sub
* 3 x Nexo PS 10 Amps

#### MICS:

* 2 x Neumann KM184
* 2 x AKG C414 XLS
* 1 x AKG C3000
* 1 x AKG D112
* 1 x Audix DP6
* 1 x Audix DP4
* 2 x Audix DP2
* 1 x DPA d:facto
* 2 x DPA d:vote 4099 with 2x piano clips, 2x mic stand clips, 2x clamp mount
* 8 x Shure SM58
* 5 x Shure SM57
* 2 x Shure Condenser BG4.1
* 1 X Shure Beta 91A
* 2 x Radial J48 Active DI
* 4 x Radial JDI Passive DI
* 2 x BSS AR 133 Active DI
* 3 x Behringer Active DI
* 2 x Emo Passive DI
* 1 x Shure SM58 Radio Mic
* 20 x Mic Stand
* 18 x Music Stand
* 2 x Guitar Stand

#### LIGHTING:

* Zero 88 Leap Frog 48ch Lighting Desk
* 4x Par 64 1kW (on Downstage Truss)
* 2 x Par 56 750w (on Front Truss)
* 4 x DTS Scena 300/500 Fresnels on FOH booms
* 4 x Blizzard Torrent 90p LED Moving Head = 575w (on Front Truss)
* 4x RGB LED Par 64 54w
* Limited Cabling

#### AV

* 1 x Panasonic PT-MZ780 Projector on Front Truss
* Accepts HDMI (no VGA) input from Stage or FOH control booth
* Retractable cinema screen (16:9)

#### AVAILABLE BACKLINE HIRE:

* Fender Twin Reverb Amp.
* Gallien Krueger head & 4 x 10” cab
* Upright Bass with pick up
* Premier Projector Kit, 18″ kick, 9″,11″,14″ toms with snare & hardware.
* Roland Keyboard Amp
* Steinway C Grand Piano (circa 1980)
* Perspex Drum Screen 180cm x 18cm

**PARKING**

* Please be advised that Triskel does not have parking spaces. We have an arrangement with Q-Park to give discounts.
* It needs to be booked in advance – instructions at the link:
* <https://triskelartscentre.ie/parking-q-park/>
* Please contact Triskel for the promo code